PSCAD 4.0.0

Settings
 {
 Id = "922310807.1043355868."
 Author = "gdi.jayas"
 Desc = ""
 Arch = "windows"
 Options = 0
 Build = 6
 Warn = 1
 Check = 15
 RunInfo = 
  {
  Fin = 0.5
  Step = 5e-005
  Plot = 0.001
  Chat = 0.001
  Brch = 0.0005
  Lat = 100
  Options = 0
  Advanced = 511
  Debug = 0
  StartFile = ""
  OFile = "noname.out"
  SFile = "noname.snp"
  SnapTime = 0.3
  Mruns = 10
  Mrunfile = 0
  StartType = 0
  PlotType = 0
  SnapType = 0
  MrunType = "mrun"
  ChangeCode = 0
  SystemMVABase = 100
  Frequency = 60
  LFoptions = 0
  G_Iterations = 5
  F_Iterations = 5
  N_Iterations = 20
  G_Precision = 0.01
  F_Precision = 0.001
  N_Precision = 0.0006
  Gause_W1 = 0.5
  Gause_W2 = 1.5
  DataFile = "noname.raw"
  }

 }

Definitions
 {
 Module("Main")
  {
  Desc = "Main Page"
  FileDate = 0
  Nodes = 
   {
   }

  Graphics = 
   {
   Rectangle(-18,-18,18,18)
   }


  Page(A/A4,Landscape,16,[640,479],100)
   {
   -Sticky-([18,18],0)
    {
    Name = ""
    Font = 1
    Bounds = 18,18,468,792
    Alignment = 0
    Style = 1
    Text = "\
PSCAD Tutorial Cases:

These cases can be found under the <PSCAD_Install_Directory>\\Examples\\Tutorial
directory.

Voltage Divider
vdiv_1.psc A simple voltage divider circuit with a resistor and a resistive source. Demonstrates how to assemble a circuit, monitor voltage and current, and run the simulation.

Fast Fourier Analysis
fft.psc Shows the use of Fast Fourier analysis component
to perform online fft on signals.

Simple AC System with a Transmission Line
simpleac.psc A Simple Ac system with transmission lines. Introduces transformers, transmission lines, and the concept of subsystems in PSCAD. simpleac_sld1.psc and simpleac_sld2.psc are two forms of single line representation of simpleac.psc.

Use of Control Arrays
pagearray.psc Demonstrates use of control arrays and how to export electrical nodes to other pages so that a circuit can be modeled on multiple pages even if you don’t have transmission lines.


Use of Slider, Switch, Button, and Dial
inputctrl.psc Shows the use of dynamic input devices: Slider, Switch, Push Button and the Dial.

Multiple Run
multirun.psc A simple control system design example to demonstrate the use of multiple run features to determine worst case overvoltages. multirun_sld.psc is single line representation of the same case.

Chatter removal
chatter.psc A simple case illustrating removal of chatter - numerical oscillation (every time step) in voltage or current which is caused by trapezoidal integration. Voltage chatter occurs whenever a disturbance is applied at a node to which only inductors are connected. Current 
chatter occurs whenever a disturbance is applied at a location where capacitors are connected in a loop.

Interpolation
interpolation.psc A simple case of GTO device using interpolation. Interpolation is an integral part of EMTDC which allows switching devices to switch at any instant of time instead of only on the regular time step grid. This allows the use of a larger time step without missing current zeroes or other switching instants.
"
    }
   -Sticky-([486,18],0)
    {
    Name = ""
    Font = 1
    Bounds = 486,18,900,720
    Alignment = 0
    Style = 1
    Text = "\
PSCAD Example Cases:

These cases can be found under the <PSCAD_Installation_directory>\\Examples directory.

hvdc\\vsc2 - Voltage Source Converter Transmission Examples

hvdc\\cigre - Cigre HVDC Benchmark Example

Matlab - Various Examples demonstrating the interface of PSCAD with Matlab.

Statcom - Statcom (Advanced SVC Facts Device) Examples

active_filters - Series and Shunt Active Filter Examples

lightning - Steep Front Overvoltages Example

ssr - IEEE SSR Benchmark Example

svc - Static Var Compensator Examples

PowerElectronics - Examples of simple power electronic circuits

PowerQuality - Examples of applications related to power quality

RTP - Demo cases for the Real Time Playback System
using the COMTRADE recorder component.

sync_machines directory
This directory has many examples to illustrate the use of synchronous machines and its accessories such as governors, exciters, stabilizers, and multi-mass models.

ind_machines directory
This directory has many examples to illustrate the use of induction machines and its accessories such as multi-mass models.

dc_machines directory
This directory has many examples to illustrate the use of dc machines and its accessories such as multi-mass models.

transformers
Includes an example of connecting single phase transformers to form a Scott connection."
    }
   }
  }
 }

